I-24056

**OC Subsection:** [[F-3681]](#3681) New OC Subsection: 06 Driving / Wipers and Washers

**Description:**

Title: Washer rear camera

Goal: Provide automatic or manual cleaning of the rear camera of the car

Context: The rear camera is dirty (the car systems cannot work correctly) during the operation of the car

Scope: Rear camera washer system

Actors: Driver

Preconditions: N/A

Triggers: It is difficult to recognize the image on the rear camera (the rear camera is dirty)

Main scenario:

1. The driver activates the rear camera cleaning function at in\_2. SWP Android by pressing once
2. The washer system is activated by spraying washer fluid into the rear camera (the washer system runs for X seconds and turns off automatically)

Postconditions:

* The rear camera is cleaned, and the image is recognized correctly.

Alternative Scenarios:

* Activation of the rear nozzle for cleaning the rear-view camera is automatically triggered every 5 times (by default) you turn on R mode. (the washer system runs for X seconds and turns off automatically)
* Driver has the flexibility to adjust this frequency:
  + Driver can customize the activation frequency in steps of 1
  + Driver can completely disable this automatic activation feature.

Exceptions: N/A

​

Requirements: N/A

**Priority:** Normal

**Type**: Use Case CF

#### Document

**Caption:** operational\_concept.Profile - 383201 Profiles settings

**Overall estimation:**

**Requirement type:** Profile

**Type**: Profile