I-23214

**OC Subsection:** [[F-3681]](#3681) New OC Subsection: 06 Driving / Wipers and Washers

**Description:**

Use Case: " Display low wash fluid level warning"

Preconditions:

* Car is on
* The driver is in the car
* The washer fluid volume sensor is functional

Main Scenario:

1. The washer fluid volume sensor indicates that the fluid is equal to 10%. <Dependency: [displaying the instruction how to fill washer fluid](#6591)>
2. The driver receives a sound and visual alert via out\_2, out\_5, or out\_25.

Postconditions:

1. The driver is notified about the low level of fluid

Alternative Scenario:

1. In B2B, an informative message will be sent to the owner or fleet manager when the washer fluid volume sensor is triggered indicating that the washer fluid volume is equal to 50%.

**Priority:** Normal

**Type**: Use Case CF